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4K60(4:2:0), HDMI2.0, HDCP2.2, POC，CEC
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*Note: This is a common user manual for all the lite version HDBaseT extenders, the chassis might be different as the different production version or it’s customized. Please refer to the real equipment.

Version: V2.0.1


1. Introduction
This lite version extender is using the HDBaseT technology, it supports no compression, no losses, no latency HDMI signal transmission. It can can work with other HDBaseT equipment, such as Sony HDBaseT projector. All the signals are transmitted by one single CAT5E/ CAT6/ CAT7 cable, for 1080P it can transmit to a distance of 70m(230ft), for 4K60Hz(4:2:0) it can up to 35m(115ft). Compatible with all the HDTV resolutions, HDCP2.2 protocol. It also supports bi-directional RS232 and IR transmission and realize the long distance control. Supports power over cable, users only need to power one side; It can be popularly used in media conferencing room, school, government, cinema and so on applications.
2. [bookmark: _Toc19797]Features
· Transmit highest quality audio and video, for 1080p can up to 220 feet and 4K60(4:2:0) can up to 115feet with Cat6/6a/7 cable
· Supports FULL HD, UHD, 3D, 4K60Hz
· HDCP2.2, HDMI2.0
· Bidirectional IR/Serial control signal transmission 
· Power over Cable (POC) locally powered over Cat5e/6 cable at either end
· Supports 7.1 DTS Master HD, Dolby True HD,
· [bookmark: _Toc14135]LED indicators, EDID pass-though
· Supports CEC control
3. Specification
	Model
	HDBaseT Lite Extender-Tx
	HDBaseT Lite Extender-Rx

	Input
	1*HDMI, 1*RS232, 1*IR-TX, 1*IR-RX
	1*HDBaseT

	Output
	1*HDBaseT
	1*HDMI, 1*RS232, 1*IR-TX, 1*IR-RX

	Protocol
	Support HDMI2.0 and compatible with HDCP2.2 

	Resolution
	1920x1200, 1680x1050, 1360x768, 1280x800, 1920x1080, 1600x900, 1366x768, 1280x720, 1024x576, 1920x1200, 1680x1050, 1360x768, 1280x800, 4096x2160@30Hz, 3840x2160@30Hz, 3840x2160@60Hz

	Color Space
	1080p: 36Bit Deep Color 4K: 24Bit True Color, 4:2:0

	Bandwidth
	10.2Gbps

	Transmission Distance
	CAT5e/6 cable: 220FT/70m(1080p60Hz, 110FT/35m(4K60Hz)

	Dimension
	115*84*16（mm）

	Weight
	120g

	Power
	AC: 100-240V 50/60Hz 1.5A Max  DC: 12V 1500mA

	Consumption
	≤11W

	Working Humidity
	10%-90%

	Working Temperature
	0℃-50℃

	Storage Temperature
	-20℃-75℃


[bookmark: _Toc10158]4. Packing
	HDBaseT Lite Extender-Rx(Receiver)
	1
	pcs

	HDBaseT Lite Extender-Tx(Transmitter)
	1
	pcs

	Power adapter(DC 12V)
	1
	pcs


[bookmark: _Toc18022]5. Panels
Transmitter
[image: ]
A: DC 12V input port         
B: POC function OFF/ON switch        
C: RJ45 output port
D: HDMI input port
E: 3-pin RS232 port
F: IR transmitter port
G: IR receiver port
H: POWER: The indicator will light up when power on
I: LINK: It will light up when the transmitter and receiver connected successfully, flecking means connection is not stable, off means the connection is failed.
J: MODE: It will flick once per second if the system runs good, on the contrary, it will be off 
or light up.



Receiver
     [image: ]
A: DC 12V input port         
B: POC function OFF/ON switch        
C: RJ45 input port
D: HDMI output port
E: 3-pin RS232 port
F: IR transmitter port
G: IR receiver port
H: POWER: The indicator will light up when power on
I: LINK: It will light up when the transmitter and receiver connected successfully, flecking means connection is not stable, off means the connection is failed.
J: MODE: It will flick once per second if the system runs good, on the contrary, it will be off 
or light up.

[bookmark: _Toc27287]6. Operation
[bookmark: _Toc19171] 6.1 Connection Diagram
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[bookmark: _Toc24911]6.2 RJ-45 connector
Suggest to use twisted shield pair 24AWG cable, the bandwidth at least 400MHz, and crystal connector.
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